Reset Procedure Control Room Osnabrück for UK wind farms

1. Turbine standstill detected, no registration of technician recorded in Rotorsoft
2. Control of status code list. Which error has caused the standstill?
3. Does one oft he following errors exist in the status code list?

* Manual brake
* Manual stop – on site
* Manual stop - remote
* Manual stop without login
* Converter emergency stop type A-F
* Emergency stop topbox
* Emergency stop nacelle
* Emergency stop converter
* Emergeny stop bottom box

Yes:

Consultation of Innogy UK control room: has a registration been recorded?

No:

Perform reset attempt and send applicable mail.

Turbine Reset by technicians onsite?